No open space is required in the R1-15 zone.