December 20, 2017

To: Weber County Engineering

From: Landmark Surveying

Subject: Drysdale Subdivision Phase 2

The review comments dated 12-12-17 from Weber County Engineering notes are addressed as follows:

A contour line has been added, the property has only about a 6” difference in elevation from back to front.

1. A 10’ P.U.E. is added along property lines.

2. Roadway is now shown.

3. Curb & Gutter will be deferred.

4. The ditch will be piped and the grade above the pipe will be a foot below the asphalt.

5. Topography note has been added.

6-9. Excavation and Storm Water Permits will be submitted at time of construction.