850 SOUTH EASEMENT DESCRIPTION

A part of the Southeast Quarter of Section 17, Township 6 North, Range 2 West, Salt Lake Base and Meridian, U.S. Survey, Weber County, Utah

Beginning at a point 233.47 feet South 01%%D06’03’ West and 1390.12 feet East; running thence to a point of curvature Southwesterly along the arc of a 20.24 foot Radius curve to the left a distance of 14.40 feet (Central Angle equals 40°44'46” and Long Chord bears South 66°59’53” West 14.10 feet to a point of tangency; thence Northeasterly along the arc of a 43.00 foot Radius curve to the Right a distance of 201.76 feet (Central Angle equals 268°49'50” and Long Chord bears North 00°54’53” East 61.43 feet to a point of tangency; thence Southeasterly along the arc of a 20.23 foot Radius curve to the right a distance of 14.43 feet (Central Angle equals 40°52'38” and Long Chord bears South 65°13’34” West 14.13 feet to a point of non-tangency; thence South 0%%D57’17” West 50.00 feet to the Point of Beginning.

Contains 5956.84 SQ. FT.

800 SOUTH EASEMENT DESCRIPTION

A part of the Southeast Quarter of Section 17, Township 6 North, Range 2 West, Salt Lake Base and Meridian, U.S. Survey, Weber County, Utah

Beginning at a point 506.14 feet South 01%%D06’03’ West and 1389.43 feet East; running thence to a point of curvature Southwesterly along the arc of a 20.19 foot Radius curve to the left a distance of 14.46 feet (Central Angle equals 41°02'27” and Long Chord bears South 67°16’00” West 14.16 feet to a point of tangency; thence Northeasterly along the arc of a 43.00 foot Radius curve to the Right a distance of 201.75 feet (Central Angle equals 268°49'49” and Long Chord bears North 01°03’42” East 61.43 feet to a point of tangency; thence Southeasterly along the arc of a 20.28 foot Radius curve to the right a distance of 14.37 feet (Central Angle equals 40°36'29” and Long Chord bears South 64°58’13” East 14.07 feet to a point of non-tangency; thence South 0%%D57’17” West 50.00 feet to the Point of Beginning.

Contains 5957.04 SQ. FT.

750 SOUTH EASEMENT DESCRIPTION

A part of the Southeast Quarter of Section 17, Township 6 North, Range 2 West, Salt Lake Base and Meridian, U.S. Survey, Weber County, Utah

Beginning at a point 778.81 feet South 01%%D06’03’ West and 1388.73 feet East; running thence to a point of curvature Southwesterly along the arc of a 20.19 foot Radius curve to the left a distance of 14.46 feet (Central Angle equals 41°02'27” and Long Chord bears South 67°16’00” West 14.16 feet to a point of tangency; thence Northeasterly along the arc of a 43.00 foot Radius curve to the Right a distance of 201.75 feet (Central Angle equals 268°49'49” and Long Chord bears North 01°03’42” East 61.43 feet to a point of tangency; thence Southeasterly along the arc of a 20.28 foot Radius curve to the right a distance of 14.37 feet (Central Angle equals 40°36'29” and Long Chord bears South 64°58’13” East 14.07 feet to a point of non-tangency; thence South 0%%D57’17” West 50.00 feet to the Point of Beginning.

Contains 5957.04 SQ. FT.

700 SOUTH EASEMENT DESCRIPTION

A part of the Southeast Quarter of Section 17, Township 6 North, Range 2 West, Salt Lake Base and Meridian, U.S. Survey, Weber County, Utah

Beginning at a point 1053.00 feet South 01%%D06’03’ West and 1293.02 feet East; running thence to a point of curvature Southwesterly along the arc of a 20.19 foot Radius curve to the left a distance of 14.47 feet (Central Angle equals 41°04'06” and Long Chord bears South 67°16’45” West 14.16 feet to a point of tangency; thence Northeasterly along the arc of a 43.00 foot Radius curve to the Right a distance of 201.75 feet (Central Angle equals 268°49'49” and Long Chord bears North 01°03’42” East 61.43 feet to a point of tangency; thence Southeasterly along the arc of a 20.28 foot Radius curve to the right a distance of 14.37 feet (Central Angle equals 40°36'43” and Long Chord bears South 64°58’16” East 14.07 feet to a point of non-tangency; thence South 0%%D56’43” West 50.00 feet to the Point of Beginning.

Contains 5957.25 SQ. FT.