Building Inspections Division review comments.

 2022- GOAL Foundation WRC 30K Special Event

1. Temporary structures shall be anchored to the ground to help prevent overturn from a wind event.
2. Portable generators shall be located outside of any structure in the open air and shall maintain the minimum required clearance to combustibles per the manufacturer’s specifications and instructions.
3. All cord-connected appliances shall be GFCI protected for personal.
4. Extension cords shall be of the grounding type and shall not be in dis-repair.
5. Extra fuel for the generator shall not be stored in a location that is a potential ignition source.
6. Temporary Tents, Umbrella and Membrane Structures shall comply with the minimum requirements of the 2018 International Building Code and the 2018 International Fire Code.

***Stan Berniche***

***Weber County Building Official***

***Building Inspections Division Director***

2380 Washington Blvd, Suite 270

Ogden, Utah 84401-1473

801-399-8760 --- Office

sberniche@webercountyutah.gov